Infrastructure

We are equipped with state-of-the-art infrastructure which encompasses all the requisite facilities for better production. Our production unit is equipped with the latest machinery which enables the smooth and effective production of material handling equipment.

Our Team

We are one of the renowned manufacturers of material handling equipment due to the support of our team of diligent and experienced professionals. Our team holds a significant position and owing to their meticulous efforts, we can successfully meet the specific demands of our clients.

Quality Assurance

Being an ISO certified company, we focus on offering the premium quality range of material handling equipment and spares. We undertake all the requisite measures to ensure international standards in our range.

Our Services

Besides providing our clients with a wide range of equipment, we also provide effective after-sales services. Assisted by a team of engineers, we provide quick assistance to our clients.

**overhead E.O.T. cranes**

We manufacture an Overhead EOT Crane which is fabricated using optimum quality raw material and components like M.S. Sheets, M.S. angles, I Beam, Motors, Brakes. Our range is designed in such a way that can bear loads ranging from up to 100 tons. These are extensively used in foundry, machine shop, engineering. We also offer customization on our range as per the specification of clients.

**overhead H.O.T. cranes**

We engineer our HOT Cranes in an I-Beam/ Box type construction for bridge girders. These are engineered in a tapered plate design for joining the end carriages to the girders thereby ensuring smooth flow of stresses. The end carriages are incorporated with L.T. Wheels.

**Jib Crane**

Jib Cranes are designed and manufactured for specific applications. Through it has limitation of working area, for applications. It proves most useful. For example, loading and unloading facility for material in open yard for loading and unloading of special purpose machine on material handling unit for C.N.C. machine kept in clean room.

**Goliath/ Gantry cranes**

Gantry / Goliath Cranes are adapted to applications where overhead runways would be very long, costly to erect, and difficult to maintain in alignment. Where the installation is only temporary, a gantry crane can be moved to a new location with less trouble or expenses than an overhead crane and its runway. Also, it is comparatively easy and inexpensive to extend the length of the runway and thus increase the working area of the crane. Most gantry crane installations are outdoors. The initial cost of a gantry crane, which may be double that of an overhead crane, must be equated against the additional cost of an overhead runway.

**Hoist**

We are Manufacture of Electric Wire Rope Hoist that is available in several models. Our Hoist is developed using optimum quality raw material such as MS Sheets, MS angles, I beam, motors, brakes etc. These are hugely demanded in machine shops, engineering industry and foundry and can be customized as per the requirement of clients.

**Pulleys, Hooks & Accessories**

**chains pulley blocks** are designed & manufactured in accordance with IS 3832 & are available in Hook suspension type: push-pull trolley type hand geared trolley type. Load chain used is graded alloy steel chain & hand chain is m.s. calibrated to relevant I.S. standards.